Title: DATA VALUE Logo__1__Graphic NOT FOUND
Author: enrico mitrovich
Company: emitrov

Product Name:   UNIREX N 2
 Revision Date:  27Jan2006
 Page  of  

______________________________________________________________________________________________________________________

MATERIAL SAFETY DATA SHEET

SECTION 1 | PRODUCT AND COMPANY IDENTIFICATION

PRODUCT
Product Name:    UNIREX N 2
Product Description:   Base Oil and Additives
Product Code:     644351-00,   97N713
Intended Use:    Grease

COMPANY IDENTIFICATION
Supplier:		EXXON MOBIL CORPORATION 
 3225 GALLOWS RD. 
FAIRFAX, VA.  22037     USA
24 Hour Health Emergency | 609-737-4411
Transportation Emergency Phone | 800-424-9300
ExxonMobil Transportation No. | 281-834-3296
MSDS Requests | 713-613-3661
Product Technical Information | 800-662-4525, 800-947-9147
MSDS Internet Address | http://www.exxon.com, http://www.mobil.com

SECTION 2 | COMPOSITION / INFORMATION ON INGREDIENTS
 
No Reportable Hazardous Substance(s) or Complex Substance(s).     

SECTION 3 | HAZARDS IDENTIFICATION
 
This material is not considered to be hazardous according to regulatory guidelines (see (M)SDS Section 15).

POTENTIAL HEALTH EFFECTS
 Low order of toxicity.  Excessive exposure may result in eye, skin, or respiratory irritation.  High-pressure injection under skin may cause serious damage. 

ENVIRONMENTAL HAZARDS
 Harmful to aquatic organisms, may cause long-term adverse effects in the aquatic environment.

NFPA Hazard ID: | Health:    0 | Flammability:   1 | Reactivity:   0
HMIS Hazard ID: | Health:    0 | Flammability:   1 | Reactivity:   0

NOTE:   This material should not be used for any other purpose than the intended use in Section 1 without expert advice. Health studies have shown that chemical exposure may cause potential human health risks which may vary from person to person.  

SECTION 4 | FIRST AID MEASURES

INHALATION
Under normal conditions of intended use, this material is not expected to be an inhalation hazard.

SKIN CONTACT
Wash contact areas with soap and water.  If product is injected into or under the skin, or into any part of the body, regardless of the appearance of the wound or its size, the individual should be evaluated immediately by a physician as a surgical emergency. Even though initial symptoms from high pressure injection may be minimal or absent, early surgical treatment within the first few hours may significantly reduce the ultimate extent of injury.

EYE CONTACT
Flush thoroughly with water.  If irritation occurs, get medical assistance.

INGESTION
First aid is normally not required. Seek medical attention if discomfort occurs.

SECTION 5 | FIRE FIGHTING MEASURES

EXTINGUISHING MEDIA
Appropriate Extinguishing Media:  Use water fog, foam, dry chemical or carbon dioxide (CO2) to extinguish flames.

Inappropriate Extinguishing Media:  Straight Streams of Water 

FIRE FIGHTING
Fire Fighting Instructions:  Evacuate area.  Prevent runoff from fire control or dilution from entering streams, sewers, or drinking water supply.  Firefighters should use standard protective equipment and in enclosed spaces, self-contained breathing apparatus (SCBA).  Use water spray to cool fire exposed surfaces and to protect personnel.  

Hazardous Combustion Products:   Aldehydes, Oxides of carbon, Sulfur oxides, Smoke, Fume, Incomplete combustion products

FLAMMABILITY PROPERTIES 
Flash Point [Method]:  >200C  (392F) [ EST. FOR OIL, ASTM D-92 (COC)]
Flammable Limits (Approximate volume % in air):  LEL:  N/D     UEL:  N/D
Autoignition Temperature:  N/D 

SECTION 6 | ACCIDENTAL RELEASE MEASURES

NOTIFICATION PROCEDURES
In the event of a spill or accidental release, notify relevant authorities in accordance with all applicable regulations. U.S. regulations require reporting releases of this material to the environment which exceed the reportable quantity or oil spills which could reach any waterway including intermittent dry creeks.  The National Response Center can be reached at (800)424-8802.

SPILL MANAGEMENT
Land Spill:  Allow spilled material to solidify and scrape up with shovels into a suitable container for recycle or disposal.  Scrape up spilled material with shovels into a suitable container for recycle or disposal.

Water Spill:  Stop leak if you can do it without risk.  Confine the spill immediately with booms.   Skim from surface.

Water spill and land spill recommendations are based on the most likely spill scenario for this material; however, geographic conditions, wind, temperature, (and in the case of a water spill) wave and current direction and speed may greatly influence the appropriate action to be taken.  For this reason, local experts should be consulted.  Note:  Local regulations may prescribe or limit action to be taken. 

ENVIRONMENTAL PRECAUTIONS
Prevent entry into waterways, sewers, basements or confined areas.

SECTION 7 | HANDLING AND STORAGE

HANDLING
 Prevent small spills and leakage to avoid slip hazard.       

Static Accumulator:   This material is not a static accumulator.

STORAGE
Do not store in open or unlabelled containers.           

SECTION 8 | EXPOSURE CONTROLS / PERSONAL PROTECTION

    

NOTE: Limits/standards shown for guidance only.  Follow applicable regulations.

ENGINEERING CONTROLS

The level of protection and types of controls necessary will vary depending upon potential exposure conditions.  Control measures to consider:
 No special requirements under ordinary conditions of use and with adequate ventilation. 

PERSONAL PROTECTION
 
Personal protective equipment selections vary based on potential exposure conditions such as applications, handling practices, concentration and ventilation.  Information on the selection of protective equipment for use with this material, as provided below, is based upon intended, normal usage.  

Respiratory Protection:   If engineering controls do not maintain airborne contaminant concentrations at a level which is adequate to protect worker health, an approved respirator may be appropriate.  Respirator selection, use, and maintenance must be in accordance with regulatory requirements, if applicable.  Types of respirators to be considered for this material include: 
 No protection is ordinarily required under normal conditions of use and with adequate ventilation.

For high airborne concentrations, use an approved supplied-air respirator, operated in positive pressure mode.  Supplied air respirators with an escape bottle may be appropriate when oxygen levels are inadequate, gas/vapor warning properties are poor, or if air purifying filter capacity/rating may be exceeded.

Hand Protection:   Any specific glove information provided is based on published literature and glove manufacturer data. Work conditions can greatly effect glove durability; inspect and replace worn or damaged gloves. The types of gloves to be considered for this material include: 
 No protection is ordinarily required under normal conditions of use.

Eye Protection:   If contact is likely, safety glasses with side shields are recommended.

Skin and Body Protection:    Any specific clothing information provided is based on published literature or manufacturer data.  The types of clothing to be considered for this material include:
 No skin protection is ordinarily required under normal conditions of use.  In accordance with good industrial hygiene practices, precautions should be taken to avoid skin contact.

Specific Hygiene Measures:   Always observe good personal hygiene measures, such as washing after handling the material and before eating, drinking, and/or smoking.  Routinely wash work clothing and protective equipment to remove contaminants.  Discard contaminated clothing and footwear that cannot be cleaned. Practice good housekeeping.

ENVIRONMENTAL CONTROLS
 See Sections  6,  7, 12, 13.

SECTION 9 | PHYSICAL AND CHEMICAL PROPERTIES

Typical physical and chemical properties are given below.   Consult the Supplier in Section 1 for additional data.

GENERAL INFORMATION
Physical State:    Solid
Form:    Semi-fluid
Color:   Green
Odor:   Characteristic
Odor Threshold:   N/D

IMPORTANT HEALTH, SAFETY, AND ENVIRONMENTAL INFORMATION
Relative Density (at 15 C ):    0.93   
Flash Point [Method]:     >200C  (392F) [ EST. FOR OIL, ASTM D-92 (COC)]
Flammable Limits (Approximate volume % in air):  LEL:  N/D     UEL:  N/D  
Autoignition Temperature:  N/D 
Boiling Point / Range:   N/D
Vapor Density (Air = 1):   N/D
Vapor Pressure:   < 0.013 kPa (0.1 mm Hg) at 20 C
Evaporation Rate (n-butyl acetate = 1):   N/D
pH:   N/A
Log Pow (n-Octanol/Water Partition Coefficient):   N/D
Solubility in Water:   Negligible
Viscosity:   113 cSt  (113 mm2/sec ) at 40 C [Base oil ]
Oxidizing Properties:  See Sections 3, 15, 16.

OTHER INFORMATION
Freezing Point:   N/D
Melting Point:   >219°C  (426°F)     
DMSO Extract (mineral oil only), IP-346:    < 3 %wt 

NOTE:  Most physical properties above are for the oil component in the material.

SECTION 10 | STABILITY AND REACTIVITY

STABILITY:  Material is stable under normal conditions.

CONDITIONS TO AVOID:  Excessive heat. High energy sources of ignition.

MATERIALS TO AVOID:   Strong oxidizers

HAZARDOUS DECOMPOSITION PRODUCTS:  Material does not decompose at ambient temperatures.

HAZARDOUS POLYMERIZATION:  Will not occur.

SECTION 11 | TOXICOLOGICAL INFORMATION

ACUTE TOXICITY
Route of Exposure | Conclusion / Remarks
Inhalation |
Toxicity (Rat): LC50 > 5000 mg/m3 | Minimally Toxic. Based on assessment of the components.
Irritation: No end point data. | Negligible hazard at ambient/normal handling temperatures. Based on assessment of the components.
Ingestion |
Toxicity (Rat): LD50 > 2000 mg/kg | Minimally Toxic. Based on test data for structurally similar materials.
Skin |
Toxicity (Rabbit): LD50 > 2000 mg/kg | Minimally Toxic. Based on test data for structurally similar materials.
Irritation (Rabbit): Data available. | Negligible irritation to skin at ambient temperatures. Based on assessment of the components.
Eye |
Irritation (Rabbit): Data available. | May cause mild, short-lasting discomfort to eyes. Based on assessment of the components.

CHRONIC/OTHER EFFECTS
 Contains:
Base oil severely refined:  Not carcinogenic in animal studies. Representative material passes IP-346, Modified Ames test, and/or other screening tests. Dermal and inhalation studies showed minimal effects; lung non-specific infiltration of immune cells, oil deposition and minimal granuloma formation. Not sensitizing in test animals.

Additional information is available by request.
 
The following ingredients are cited on the lists below:  None.

--REGULATORY LISTS SEARCHED--
1 = NTP CARC | 3 = IARC 1 | 5 = IARC 2B
2 = NTP SUS | 4 = IARC 2A | 6 = OSHA CARC

SECTION 12 | ECOLOGICAL INFORMATION

The information given is based on data available for the material, the components of the material, and similar materials.

ECOTOXICITY   
             Material -- Expected to be harmful to aquatic organisms. May cause long-term adverse effects in the aquatic environment.

MOBILITY 
             Base oil component -- Low solubility and floats and is expected to migrate from water to the land.  Expected to partition to sediment and wastewater solids. 

PERSISTENCE AND DEGRADABILITY
Biodegradation: 
             Base oil component --  Expected to be inherently biodegradable   

BIOACCUMULATION POTENTIAL 
             Base oil component -- Has the potential to bioaccumulate, however metabolism or physical properties may reduce the bioconcentration or limit bioavailability.

    
 
SECTION 13 | DISPOSAL CONSIDERATIONS
 
Disposal recommendations based on material as supplied.  Disposal must be in accordance with current applicable laws and regulations, and material characteristics at time of disposal. 

DISPOSAL RECOMMENDATIONS
 Suitable routes of disposal are supervised incineration, preferentially with energy recovery, or appropriate recycling methods in accordance with applicable regulations and material characteristics at the time of disposal. 
 
REGULATORY DISPOSAL INFORMATION
 RCRA Information: Disposal of unused product may be subject to RCRA regulations (40 CFR 261).  Disposal of the used product may also be regulated due to ignitability, corrosivity, reactivity or toxicity as determined by the Toxicity Characteristic Leaching Procedure (TCLP).  Potential RCRA characteristics:
TCLP (BARIUM)

 Empty Container Warning PRECAUTIONARY LABEL TEXT:  Empty containers may retain residue and can be dangerous.  DO NOT PRESSURIZE, CUT, WELD, BRAZE, SOLDER, DRILL, GRIND OR EXPOSE SUCH CONTAINERS TO HEAT, FLAME, SPARKS, STATIC ELECTRICITY, OR OTHER SOURCES OF IGNITION; THEY MAY EXPLODE AND CAUSE INJURY OR DEATH.  Do not attempt to refill or clean container since residue is difficult to remove.  Empty drums should be completely drained, properly bunged and promptly returned to a drum reconditioner.  All containers should be disposed of in an environmentally safe manner and in accordance with governmental regulations.

SECTION 14 | TRANSPORT INFORMATION

LAND (DOT) :  Not Regulated for Land Transport
                   
LAND (TDG) :  Not Regulated for Land Transport

SEA (IMDG) :  Not Regulated for Sea Transport according to IMDG-Code

AIR (IATA) :  Not Regulated for Air Transport

SECTION 15 | REGULATORY INFORMATION

OSHA HAZARD COMMUNICATION STANDARD:   When used for its intended purposes, this material is not classified as hazardous in accordance with OSHA 29 CFR 1910.1200.

NATIONAL CHEMICAL INVENTORY LISTING:   DSL, EINECS, TSCA

EPCRA:  This material contains no extremely hazardous substances.

SARA (311/312) REPORTABLE HAZARD CATEGORIES:   None.

SARA (313) TOXIC RELEASE INVENTORY:  This material contains no chemicals subject to the supplier notification requirements of the SARA 313 Toxic Release Program.

The Following Ingredients are Cited on the Lists Below:*  
Chemical Name | CAS Number | List Citations
DIPHENYLAMINE | 122-39-4 | 5, 9

--REGULATORY LISTS SEARCHED--
1 = ACGIH ALL | 6 = TSCA 5a2 | 11 = CA P65 REPRO | 16 = MN RTK
2 = ACGIH A1 | 7 = TSCA 5e | 12 = CA RTK | 17 = NJ RTK
3 = ACGIH A2 | 8 = TSCA 6 | 13 = IL RTK | 18 = PA RTK
4 = OSHA Z | 9 = TSCA 12b | 14 = LA RTK | 19 = RI RTK
5 = TSCA 4 | 10 = CA P65 CARC | 15 = MI 293 |

Code key: CARC=Carcinogen; REPRO=Reproductive

* EPA recently added new chemical substances to its TSCA Section 4 test rules.  Please contact the supplier to confirm whether the ingredients in this product currently appear on a TSCA 4 or TSCA 12b list.

SECTION 16 | OTHER INFORMATION
N/D = Not determined, N/A = Not applicable

THIS SAFETY DATA SHEET CONTAINS THE FOLLOWING REVISIONS:
No revision information is available.   
-----------------------------------------------------------------------------------------------------------------------------------------------------               
-----------------------------------------------------------------------------------------------------------------------------------------------------
The information and recommendations contained herein are, to the best of ExxonMobil's knowledge and belief, accurate and reliable as of the date issued.  You can contact ExxonMobil to insure that this document is the most current available from ExxonMobil.  The information and recommendations are offered for the user's consideration and examination.  It is the user's responsibility to satisfy itself that the product is suitable for the intended use.  If buyer repackages this product, it is the user's responsibility to insure proper health, safety and other necessary information is included with and/or on the container.  Appropriate warnings and safe-handling procedures should be provided to handlers and users.  Alteration of this document is strictly prohibited.  Except to the extent required by law, re-publication or retransmission of this document, in whole or in part, is not permitted.  The term, "ExxonMobil" is used for convenience, and may include any one or more of ExxonMobil Chemical Company, Exxon Mobil Corporation, or any affiliates in which they directly or indirectly hold any interest.

-----------------------------------------------------------------------------------------------------------------------------------------------------
Internal Use Only |
MHC:  0, 0, 0, 0, 0, 0 | PPEC:   A

 DGN:  2031341XUS  (553418)
-----------------------------------------------------------------------------------------------------------------------------------------------------
Copyright 2002 Exxon Mobil Corporation, All rights reserved